|  |
| --- |
| **KENTUCKY SWIMMING POOL SAFETY CHECKLIST** |
| **MEET:** |  | **DATE** |  |
|  |  |  |  |
| **DECK/RESTROOMS**  | **YES** | **NO** | **ACTION** |
| Safety equipment (first aid) |  |  |  |
| Backboard/AED |  |  |  |
| Telephone, emergency # |  |  |  |
| Posted rules |  |  |  |
| Deck condition/surface |  |  |  |
| Standing water |  |  |  |
| No glass/sharp object |  |  |  |
| Electrical safety |  |  |  |
| Restrooms clean/secure |  |  |  |
| Restrooms monitoring |  |  |  |
| Cell/video sign posted |  |  |  |
| Lighting |  |  |  |
| Entry /exit marked/secure |  |  |  |
| Emergency plan in place |  |  |  |
| Trash receptacles |  |  |  |
| Report of Occurrence |  |  |  |
| Meet Marshall plan |  |  |  |
| Posted warm up schedule |  |  |  |
| Shower/restroom security |  |  |  |
| Coach/adult ID |  |  |  |
| Deck Security/access |  |  |  |

|  |  |  |  |
| --- | --- | --- | --- |
| **POOL** | **YES** | **NO** | **ACTION** |
| Lane width 6-9 feet |  |  |  |
| Water Temp 25-28 degrees C / 77-82.4 degrees F |  |  |  |
| End wall no slip without protrusions, windows or inlets |  |  |  |
| Markings on end wall and approaching wall |  |  |  |
| Deck not more than 12” above water surface, non slip |  |  |  |
| 15M mark – 49’ 2.55” |  |  |  |
| Remove ladders, obstacles |  |  |  |
| Blocks – stable, non-slip (top 20-34” slope not greater than 10 degrees) |  |  |  |
| Block LCM, SCM – 20” to 27.5” above surface of pool |  |  |  |
| Water is at overflow rim |  |  |  |
| Backstroke flags at least 3 pennants – 5 yards from edge in 25-yard pool |  |  |  |
| Backstroke flags at least 3 pennants – 5M in 25/50-meter pool (16’ 5“) |  |  |  |
| Backstroke flags 5’ 11” – 8’ 3” above water |  |  |  |
| Pool depth 6’ minimum for teaching racing starts |  |  |  |
| Pool depth minimum 4’ (from 3’ 3” out to 16’ 5” from start) for competition |  |  |  |
| Course 50M – 164” o.5”, 25M 82’ .25” |  |  |  |
| Must have certified course to achieve world or American records |  |  |  |
|  |  |  |  |